SECTION 13 48 13

Green Glue Viscoelastic Damping Compound

**PART 1 GENERAL**

1. **SECTION INCLUDES**
   1. Green Glue viscoelastic damping compound.
2. **SUBMITTALS**
   1. Product Data: Manufacturer’s data sheet and installation instructions.
3. **QUALITY ASSURANCE**
   1. Qualifications:
      1. Manufacturers: Provide viscoelastic damping compound from a single manufacturer.
      2. Installers: Utilize an installer having demonstrated experience on projects of comparable size and complexity.
4. **DELIVERY, STORAGE, AND HANDLING**
   1. Storage and Handling Requirements:
      1. Store tubes indoors in a clean, cool, dry place, and out of direct sunlight.
      2. Store tubes in a space where the ambient temperature and humidity conditions are being maintained at the levels indicated for the project when occupied for its intended use.
5. **SITE CONDITIONS**
   1. Ambient Conditions:
      1. Maintain ambient temperature and humidity conditions at levels indicated for the project when occupied for its intended use.
      2. Do not install product under environmental conditions outside manufacturer’s recommended limits.
6. **WARRANTY**
   1. Provide manufacturer’s written product warranty per Section 01 77 00 – Closeout Procedures.

**PART 2 PRODUCTS**

1. **MANUFACTURERS**
   1. Acoustical Surfaces, Inc., 123 Columbia Court N, Chaska, MN 55318.  
      Phone: 952-448-5300. Fax: 952-448-2613. Website: www.acousticalsurfaces.com
2. **DESCRIPTION**
   1. Product: Green Glue viscoelastic damping compound by Acoustical Surfaces, Inc.
   2. Product Information:
      1. Composition: Viscoelastic damping compound
      2. Size: 28 oz. tube
      3. Coverage: Approximately 16 sqft per tube at full coverage
      4. Technical Specs: Refer to manufacturer data sheet for technical specifications and  
          performance

**PART 3 EXECUTION**

1. **EXAMINATION**
2. Verification of Conditions:
3. All wet work in the installation area must be complete, cured, and dry prior to installation.
4. **INSTALLATION**
5. Comply with manufacturer’s instructions and recommendations for installation of wall panels and with industry standards.

END OF SECTION